{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["东校园菜市生鲜店装修"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"东校园菜市生鲜店装修","index":0,"n_rows":76,"n_cols":6,"rows_kept":76,"merged":[[0,0,0,5],[1,0,3,0],[1,1,3,1],[1,2,3,2],[1,3,3,3],[1,4,3,4],[1,5,3,5],[13,1,13,2],[23,1,23,2],[47,0,48,0],[47,1,48,1],[75,0,75,5]],"flags":["formulas_cached_only"]}
["东校园菜市生鲜店装修工程 "]
["序号","项目名称","具体做法、材料规格及技术参数","参考品牌","工程量","单位"]
[]
[]
[null,"拆改工程"]
[1,"墙体拆除","人工拆除原有砖墙（包含墙面瓷砖），废渣清理成堆，放到指定的位置。",null,{"v":4.2648,"d":"4.26"},"m³"]
[2,"外墙瓷砖拆除","人工拆除墙面瓷砖，废渣清理成堆，放到指定的位置。",null,11.05,"㎡"]
[3,"室内墙面沥青清除","人工清理原有墙面沥青，废渣清理成堆，放到指定的位置。",null,86.94,"㎡"]
[4,"门头过梁","宽同墙宽，120高C20钢筋混凝土过梁",null,0.25,"m³"]
[5,"结构柱","规格500*500mm，砌砖到梁底，（柱与旧墙体间需植筋连接，间距500mm，植筋直径为8mm）",null,1.55,"m³"]
[6,"室内封堵窗洞","砖封堵原墙面洞口",null,2.88,"㎡"]
[7,"拆除现场遗留废料","角架、木方等",null,{"v":3,"d":"3.00"},"m³"]
[8,"室外篷布移位","将固定于墙上的篷布移动到屋顶固定",null,{"v":1.5,"d":"1.50"},"人工"]
[null,"合计"]
[null,"钢筋结构工程"]
[1,"人工开挖基坑","打凿柱基，尺寸为1300*1300*1100mm",null,{"v":3.718,"d":"3.72"},"m³"]
[2,"垫层","强度等级:C10，尺寸1300*1300*100mm",null,{"v":0.338,"d":"0.34"},"m³"]
[3,"柱基础混凝土","强度等级:C25，基底尺寸1200*1200*450mm",null,{"v":1.296,"d":"1.30"},"m³"]
[4,"柱基础模板","1.胶合板模板、木模板的制作。\n2.模板安装、拆除、整理堆放及场内外运输。",null,{"v":17.4,"d":"17.40"},"㎡"]
[5,"柱混凝土","强度等级:C25，柱尺寸500*500*3150mm",null,{"v":1.863,"d":"1.86"},"m³"]
[6,"直径18钢筋","HRB335带肋钢筋，部位：柱子纵筋",null,{"v":0.166,"d":"0.17"},"T"]
[7,"直径10钢筋","HRB335带肋钢筋，部位：基础纵横受力筋",null,{"v":0.032084,"d":"0.03"},"T"]
[8,"直径8钢筋","HPB235广源钢筋，部位:柱子箍筋",null,{"v":0.0316,"d":"0.03"},"T"]
[null,"合计"]
[null,"天花工程"]
[1,"室内铝扣板吊顶","吊顶形式、吊杆规格、高度:不上人型 平面，龙骨材料种类、规格、中距:600×600Ф 8吊杆轻钢龙骨架，面层材料品种、规格:0.8mm厚600×600铝扣板",null,60.39,"㎡"]
[null,null,"合计"]
[null,"墙面工程"]
[1,"室内墙面挂网抹灰","1、钉钢丝网一层，墙面刷素水泥浆一道；\n2、9厚1:3水泥砂浆打底找毛；\n3、8厚1:2.5水泥砂浆找平，海绵拉细毛",null,{"v":89.975,"d":"89.98"},"㎡"]
[2,"室外墙面抹灰","1、9厚1:3水泥砂浆打底找毛；\n2、8厚1:2.5水泥砂浆找平，海绵拉细毛",null,{"v":20.2675,"d":"20.27"},"㎡"]
[3,"室内墙面贴砖","纯白瓷砖、瓷砖胶水泥膏结合层、表面拉毛处理、刷背胶人工及辅材费。","优于或相当于“宏宇陶瓷”、“新中源陶瓷 ”品牌的中档瓷砖。",{"v":86.375,"d":"86.38"},"㎡"]
[4,"室外墙面刮腻子","基层处理、水性腻子批底灰,砂纸打磨平整。",null,{"v":24.0175,"d":"24.02"},"㎡"]
[5,"室外墙面乳胶漆","立邦面漆、底漆滚涂 ，一遍底漆、二遍面漆","选用相当于或优于立邦净味120二合一墙面漆",{"v":24.0175,"d":"24.02"},"㎡"]
[null,null,"合计"]
[null,"地面工程"]
[1,"地砖（灰色）","规格：800*800，瓷砖1:3干硬性水泥砂浆、水泥膏结合层、人工及辅材费，品牌优于或相当于“宏宇陶瓷”、“新中源陶瓷 ”品牌的中档瓷砖\n","优于或相当于“宏宇陶瓷”、“新中源陶瓷 ”品牌的中档瓷砖。",60.39,"㎡"]
[2,"入户石材门槛石（规格：800mm*实际宽度）","“爵士黑”大理石、1:3干硬性水泥砂浆、水泥膏结合层、人工及辅材费。 ","优于或相当于“宏宇陶瓷”、“新中源陶瓷 ”品牌的中档瓷砖。",6.35,"m"]
[null,null,"合计"]
[null,"电箱、检修口"]
[1,"强电电箱","16位空开强电箱，漏电保护器及空开",null,{"v":1,"d":"1.00"},"套"]
[null,null,"合计"]
[null,"门窗部分"]
[1,"电动铝合金卷帘门","0.8厚铝合金，颜色为白色",null,{"v":22.392,"d":"22"},"㎡"]
[2,"卷帘门电动装置","额定功率不低于250w，提升力不小于450kg.f",null,3,"组"]
[null,null,"合计"]
[null,"强、弱电铺设"]
[1,"灯具电路","室内照明、灯具电路，ZR-BV-0.45/0.75kV-2.5mm2\n","相当于或优于“桂林国际（穿山牌）”“南宁银杉（银杉牌）”品牌",{"v":60,"d":"60.00"},"m"]
[2,"插座电路","插座，型号： ZR-BV-0.45/0.75kV-4mm2\n","相当于或优于“桂林国际（穿山牌）”“南宁银杉（银杉牌）”品牌",{"v":169.845,"d":"169.85"},"m"]
[null,null,"净菜柜，型号： ZR-BV-0.45/0.75kV-6mm2\n","相当于或优于“桂林国际（穿山牌）”“南宁银杉（银杉牌）”品牌",41.04,"m"]
[3,"弱电敷设","接入弱电箱,超6类网线",null,{"v":15,"d":"15.00"},"m"]
[4,"主电源","接入电房，型号WDZB-YJY-5*16mm2","相当于或优于“桂林国际（穿山牌）”“南宁银杉（银杉牌）”品牌",{"v":20,"d":"20.00"},"m"]
[5,"PVC矩形30线槽","强电系统分支管、线、钢丝软管、盒及附件的供应及安装，规格30*10mm",null,{"v":20,"d":"20.00"},"m"]
[6,"PVC矩形20线槽","强电系统分支管、线、钢丝软管、盒及附件的供应及安装，规格20*10mm",null,{"v":143.435,"d":"143.44"},"m"]
[null,null,"合计"]
[null,"开关、插座"]
[1,"LED面板灯","尺寸600×600mm， 36W，安装方式:嵌入吊顶安装。","相当于或优于广东三雄极光照明股份有限公司（三雄·极光）、雷士 照明控股有限公司 （NVC雷士照明）、欧普照明股份有限公司（欧普照明）",15,"套"]
[2,"明装二、三级插座","二、三级插座，16A \n","相当于或优于西蒙电气（中国）有限公司、TCL罗格朗国际电工（惠州）有限公司产品",2,"套"]
[3,"二、三级连体拨启式方形铜面地脚插座","材质：黄铜+阻燃PC材料，16A","相当于或优于西蒙电气（中国）有限公司、TCL罗格朗国际电工（惠州）有限公司产品",4,"套"]
[4,"地插底盒","材质：铁合金；尺寸：100*100mm",null,4,"套"]
[null,null,"合计"]
[null,"给排水铺设"]
[1,"冷水PPRDe20型管安装","连接方式：粘接连接，工作压力：1.6MPa，含管道消毒冲洗、水压试验。","品牌相当于或优于广东联塑科技实业有限公司（L&S牌）、广东雄塑科技实业有 限公司（X&S牌）、日丰企业集团有限公司(日丰牌)产品",{"v":10.14,"d":"10"},"m"]
[2,"水路PPR热水De15型管安装","连接方式：粘接连接，工作压力：1.6MPa，含管道消毒冲洗、水压试验。","品牌相当于或优于广东联塑科技实业有限公司（L&S牌）、广东雄塑科技实业有 限公司（X&S牌）、日丰企业集团有限公司(日丰牌)产品",1,"m"]
[3,"排污PVC-U De50型管安装","连接方式：粘接连接，含闭水试验，","品牌相当于或优于广东联塑科技实业有限公司（L&S牌）、广东雄塑科技实业有 限公司（X&S牌）、日丰企业集团有限公司(日丰牌)产品",3,"m"]
[4,"排污PVC-U De75型管安装","连接方式：粘接连接，含闭水试验，","品牌相当于或优于广东联塑科技实业有限公司（L&S牌）、广东雄塑科技实业有 限公司（X&S牌）、日丰企业集团有限公司(日丰牌)产品",13,"m"]
[null,null,"合计"]
[null,"其他费"]
[1,"施工围档","施工护栏 彩钢板 型钢 高1.76m",null,29.92,"㎡"]
[2,"原现场遗留垃圾外运","人工装渣土、加盖自卸汽车建筑垃圾，运距:15KM",null,11.78,"m³"]
[3,"施工建筑垃圾外运","人工装渣土、加盖自卸汽车建筑垃圾，运距:15KM",null,11.78,"m³"]
[4,"成品保护","包含人工安装及辅材费用",null,60.39,"㎡"]
[5,"其他措施费","钢管满堂脚手架",null,60.39,"㎡"]
[null,null,"合计"]
[null,"不可预见费",null,null,{"v":1,"d":"1.00"},"项"]
[null,null,"总计"]
["备注：包干单价包含人工费、材料费、机械台班费、管理费、措施费、利润、规费、税费、风险费用等其他一切相关费用。"]